Пример установки Micro/RSX V1 в SimH.
Установить в Ersatz-11 не удалось.



PDP-11 simulator V3.8-1
sim> set cpu 1m   
Disabling CR
Disabling RK
Disabling HK
Disabling TM
sim> set tto 7b
sim> at rq0 microrsx.dsk
RQ: creating new file
sim> set rq1 rx50 lock  
sim> at rq1 ursx1ins.dsk
sim> set rq2 rx50 lock  
sim> at rq2 ursx1os1.dsk
sim> b rq1



Micro/RSX   


  Micro/RSX Installation/Backup Procedure

         This is the Micro/RSX installation and backup procedure.
         You can use this procedure to either:

            I -- Install your Micro/RSX operating system
                 for the first time

            B -- Back up files from the fixed disk

            R -- Restore files to the fixed disk

            D -- Duplicate diskettes

         Type I for install, B for back up, R for restore, or
         D for duplicate, then press the RETURN key.

         Which do you want to do? I


  Micro/RSX Installation Procedure

         Welcome to the Micro/RSX installation procedure.

         The installation consists of:

            o  Preparing the fixed disk for use

            o  Copying your Micro/RSX operating system from
               the diskettes to the fixed disk

            o  Starting up your Micro/RSX operating system
               on the fixed disk

         These three steps will take about 30 minutes.

         To continue, press the RETURN key...


         The first step is preparing the fixed disk for use.

         This will take about 4 minutes.  The terminal will beep
         when done.

         You might want to take this time to read the next three
         sections in the installation guide:

            The Micro/RSX Installation Procedure -- What Is It?

            Logging in to Micro/RSX

            Correcting Possible Errors

         Please wait...


         The preparation of the fixed disk is complete.

         The next step is copying your Micro/RSX operating system
         from the diskettes to the fixed disk.

         Find the six diskettes labeled OPERATING SYSTEM and
         the diskette labeled HELP FILES.

         The diskette labeled EXTENDED ERROR LOGGING is not needed
         at this time.

         When you have the seven diskettes, press the RETURN key...


         You will be guided through this part of the installation
         by instructions on this terminal.  All you need to do is
         follow them carefully when they appear.

         You will be asked to insert the first diskette into
         drive 2 and to wait while the contents of the diskette
         are copied to the fixed disk.

         Then you will be asked to remove that diskette and
         insert the next one.

         You will be asked to repeat this sequence until all
         seven diskettes have been copied.

         To continue reading, press the RETURN key...


         Insert and remove diskettes from drive 2 only.  Do not
         remove the installation diskette in drive 1.

         For the FLOOR-STAND model, drive 2 is the right-hand
         drive.

         For the RACK-MOUNT or TABLE-TOP model, drive 2 is the
         bottom drive.

         Before opening the drive door to remove or insert a
         diskette, make sure both active drive lights are off
         and both drives are quiet.

         To continue reading, press the RETURN key...


         Insert the first diskette, labeled OPERATING SYSTEM  1 OF 6,
         into drive 2 as follows:

         1. ALIGN the orange arrow on the diskette with the orange bar
            on drive 2.  Note that this alignment is OPPOSITE from the
            way you inserted the installation diskette in drive 1.

         2. For the FLOOR-STAND model, make sure the diskette label
            faces right and the write-protect tab is up.

            For the RACK-MOUNT or TABLE-TOP model, make sure the diskette
            label faces down and the write-protect tab is on the right.

         3. SLIDE the diskette into drive 2 and CLOSE the door gently.

         When you have inserted the diskette, press the RETURN key...


         Thank you.  Now copying the first diskette to the fixed
         disk.

         This will take a little more than 1 minute.

         Please wait...


         That diskette is copied.  Please remove it and insert
         the second diskette, labeled

               OPERATING SYSTEM  2 OF 6

         into drive 2.

         When you have inserted the diskette, press the RETURN key...
(нажать Ctrl/E)
Simulation stopped, PC: 005226 (BR 5174)
sim> det rq2
sim> at rq2 ursx1os2.dsk
sim> c
(нажать Enter)


         Thank you.  Now copying the second diskette to the fixed
         disk.

         This will take about 1 minute.

         Please wait...


         That diskette is copied.  Please remove it and insert
         the third diskette, labeled

               OPERATING SYSTEM  3 OF 6

         into drive 2.

         When you have inserted the diskette, press the RETURN key...
(нажать Ctrl/E)
Simulation stopped, PC: 005226 (BR 5174)
sim> det rq2
sim> at rq2 ursx1os3.dsk
sim> c
(нажать Enter)


         Thank you.  Now copying the third diskette to the fixed
         disk.

         This will take about 1 minute.

         Please wait...


         That diskette is copied.  Please remove it and insert
         the fourth diskette, labeled

               OPERATING SYSTEM  4 OF 6

         into drive 2.

         When you have inserted the diskette, press the RETURN key...
(нажать Ctrl/E)
Simulation stopped, PC: 005226 (BR 5174)
sim> det rq2
sim> at rq2 ursx1os4.dsk
sim> c
(нажать Enter)


         Thank you.  Now copying the fourth diskette to the fixed
         disk.

         This will take about 1 minute.

         Please wait...


         That diskette is copied.  Please remove it and insert
         the fifth diskette, labeled

               OPERATING SYSTEM  5 OF 6

         into drive 2.

         When you have inserted the diskette, press the RETURN key...
(нажать Ctrl/E)
Simulation stopped, PC: 005226 (BR 5174)
sim> det rq2
sim> at rq2 ursx1os5.dsk
sim> c
(нажать Enter)


         Thank you.  Now copying the fifth diskette to the fixed
         disk.

         This will take about 1 minute.

         Please wait...


         That diskette is copied.  Please remove it and insert
         the sixth diskette, labeled

               OPERATING SYSTEM  6 OF 6

         into drive 2.

         When you have inserted the diskette, press the RETURN key...
(нажать Ctrl/E)
Simulation stopped, PC: 005226 (BR 5174)
sim> det rq2
sim> at rq2 ursx1os6.dsk
sim> c
(нажать Enter)


         Thank you.  Now copying the sixth diskette to the fixed
         disk.

         This will take about 1 minute.

         Please wait...


         That diskette is copied.  Please remove it and insert
         the last diskette, labeled

               HELP FILES

         into drive 2.

         When you have inserted the diskette, press the RETURN key...
(нажать Ctrl/E)
Simulation stopped, PC: 005226 (BR 5174)
sim> det rq2
sim> at rq2 ursx1hel.dsk
sim> c
(нажать Enter)


         Thank you.  Now copying the last diskette to the fixed
         disk.

         This will take about 3 minutes.

         Please wait...


         The last diskette is copied.  Please remove it from
         drive 2 and close the drive door.

         When you have removed the diskette, press the RETURN key...
(нажать Ctrl/E)
Simulation stopped, PC: 005226 (BR 5174)
sim> det rq2
sim> c
(нажать Enter)


         The final step is starting up your Micro/RSX operating
         system that was just copied onto the fixed disk.

         The screen will go blank for about 30 seconds, and then
         you will see the normal start-up procedure for your
         Micro/RSX operating system.

         To start up your Micro/RSX system, press the RETURN key...



Micro/RSX   
$

   Micro/RSX system startup procedure

          Copyright (C) 1984 by Digital Equipment Corporation

          Please enter the time and date. The month name must
          be three characters long (example: SEP) and the time
          must be in 24-hour format (example: 13:00 for 1:00 p.m.).
          After entering the time and date press the return key.
          Example: 13:55 30-MAR-84

          Time and date : 31-MAY-99 23:45


          Startup will take between one and three minutes to complete.


*************************************************************************
*                                                                       *
*       Please remove the installation diskette from drive 1            *
*       and close the drive door.                                       *
*                                                                       *
*************************************************************************
Press return to continue 
(нажать Ctrl/E)
Simulation stopped, PC: 010222 (BR 10170)
sim> det rq1
sim> 
sim> c
(нажать Enter)


*************************************************************************
*                                                                       *
*       Congratulations!  Your Micro/RSX operating system is            *
*       installed and ready for use.  You can now log in and            *
*       begin to use the system.                                        *
*                                                                       *
*       If you are not familiar with the Micro/RSX operating            *
*       system, you should read the Introduction to Micro/RSX.          *
*       It includes a self-paced instruction course to introduce        *
*       you to the system.                                              *
*                                                                       *
*       To log in, see the section entitled Logging in to Micro/RSX     *
*       in the installation guide.                                      *
*                                                                       *
*       After you log in, you can install any optional software         *
*       you may have purchased.  See the installation guide in          *
*       your optional software box.                                     *
*                                                                       *
*************************************************************************
Press return to continue


*************************************************************************
*                                                                       *
*                    Installation of your Micro/RSX                     *
*                                                                       *
*              operating system has completed successfully              *
*                                                                       *
*************************************************************************

$ 
$ 
Have a Good Evening
31-MAY-99 23:45 TT0:  logged off MICRO  
$ HEL MICRO/RSX

Micro/RSX    V1.0  BL7.0  [1,54] System     MICRO 
31-MAY-99 23:45  Logged on Terminal TT0:  as PRV1

Good Evening

 
	*********************************************************
	*                                                       *
	*                Welcome to Micro/RSX                   *
	*              Version 1  Base level 7.0                *
	*                                                       *
	*            This is file LB:[1,2]LOGIN.TXT             *
	*                                                       *
	*********************************************************
 
$ @LB:[1,2]SYSLOGIN.CMD
$ @ <EOF>
$ 
