PDP-11 simulator V3.6-1
sim> set cpu 11/45
Disabling XQ
sim> set rp0 rp04
sim> att rp0 unixv7.dsk
RP: creating new file
Create bad block table on last track? [N] y
sim> set tm0 locked
sim> att tm0 unixv7.tap
sim> boo tm0
Boot
: tm(0,3)
file sys size: 5000
file system: hp(0,0)
isize = 1600
m/n = 3 500
Exit called
Boot
: tm(0,4)
Tape? tm(0,5)
Disk? hp(0,0)
Last chance before scribbling on disk. 
End of tape
Boot
: hp(0,0)hptmunix
mem = 177344
# MV HPTMUNIX UNIX
# CD /DEV
# MAKE RP04
/ETC/MKNOD RP0 B 6 0
/ETC/MKNOD SWAP B 6 1
/ETC/MKNOD RP3 B 6 6
/ETC/MKNOD RRP0 C 14 0
/ETC/MKNOD RRP3 C 14 6
CHMOD GO-W RP0 SWAP RP3 RRP0 RRP3
# MAKE TM
/ETC/MKNOD MT0 B 3 0
/ETC/MKNOD RMT0 C 12 0
/ETC/MKNOD NRMT0 C 12 128
CHMOD GO+W MT0 RMT0 NRMT0
# /ETC/MKFS /DEV/RP3 153406
ISIZE = 49088
M/N = 3 500
# DD IF=/DEV/NRMT0 OF=/DEV/NULL BS=20B FILES=6
202+80 RECORDS IN
202+75 RECORDS OUT
# RESTOR RF /DEV/RMT0 /DEV/RP3
LAST CHANCE BEFORE SCRIBBLING ON /DEV/RP3. 
END OF TAPE
# /ETC/MOUNT /DEV/RP3 /USR 
# DD IF=/USR/MDEC/HPUBOOT OF=/DEV/RP0 COUNT=1
0+1 RECORDS IN
0+1 RECORDS OUT
#
